/*
    FreeRTOS V7.0.2 - Copyright (C) 2011 Real Time Engineers Ltd.
	

    ***************************************************************************
     *                                                                       *
     *    FreeRTOS tutorial books are available in pdf and paperback.        *
     *    Complete, revised, and edited pdf reference manuals are also       *
     *    available.                                                         *
     *                                                                       *
     *    Purchasing FreeRTOS documentation will not only help you, by       *
     *    ensuring you get running as quickly as possible and with an        *
     *    in-depth knowledge of how to use FreeRTOS, it will also help       *
     *    the FreeRTOS project to continue with its mission of providing     *
     *    professional grade, cross platform, de facto standard solutions    *
     *    for microcontrollers - completely free of charge!                  *
     *                                                                       *
     *    >>> See http://www.FreeRTOS.org/Documentation for details. <<<     *
     *                                                                       *
     *    Thank you for using FreeRTOS, and thank you for your support!      *
     *                                                                       *
    ***************************************************************************


    This file is part of the FreeRTOS distribution.

    FreeRTOS is free software; you can redistribute it and/or modify it under
    the terms of the GNU General Public License (version 2) as published by the
    Free Software Foundation AND MODIFIED BY the FreeRTOS exception.
    >>>NOTE<<< The modification to the GPL is included to allow you to
    distribute a combined work that includes FreeRTOS without being obliged to
    provide the source code for proprietary components outside of the FreeRTOS
    kernel.  FreeRTOS is distributed in the hope that it will be useful, but
    WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY
    or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License for
    more details. You should have received a copy of the GNU General Public
    License and the FreeRTOS license exception along with FreeRTOS; if not it
    can be viewed here: http://www.freertos.org/a00114.html and also obtained
    by writing to Richard Barry, contact details for whom are available on the
    FreeRTOS WEB site.

    1 tab == 4 spaces!

    http://www.FreeRTOS.org - Documentation, latest information, license and
    contact details.

    http://www.SafeRTOS.com - A version that is certified for use in safety
    critical systems.

    http://www.OpenRTOS.com - Commercial support, development, porting,
    licensing and training services.
*/

#ifndef INC_FREERTOS_H
#define INC_FREERTOS_H


/*
 * Include the generic headers required for the FreeRTOS port being used.
 */
#include <stddef.h>

/* Basic FreeRTOS definitions. */
#include "projdefs.h"

/* Application specific configuration options. */
#include "FreeRTOSConfig.h"

/* Definitions specific to the port being used. */
#include "portable.h"


/* Defines the prototype to which the application task hook function must
conform. */
typedef portBASE_TYPE (*pdTASK_HOOK_CODE)( void * );


extern int ulSetInterruptMaskFromISR( void );
extern void vClearInterruptMaskFromISR( int ulMask );


/*
 * Check all the required application specific macros have been defined.
 * These macros are application specific and (as downloaded) are defined
 * within FreeRTOSConfig.h.
 */

#ifndef configUSE_PREEMPTION
	#error Missing definition:  configUSE_PREEMPTION should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef configUSE_IDLE_HOOK
	#error Missing definition:  configUSE_IDLE_HOOK should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef configUSE_TICK_HOOK
	#error Missing definition:  configUSE_TICK_HOOK should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef configUSE_CO_ROUTINES
	#error  Missing definition:  configUSE_CO_ROUTINES should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef INCLUDE_vTaskPrioritySet
	#error Missing definition:  INCLUDE_vTaskPrioritySet should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef INCLUDE_uxTaskPriorityGet
	#error Missing definition:  INCLUDE_uxTaskPriorityGet should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef INCLUDE_vTaskDelete		
	#error Missing definition:  INCLUDE_vTaskDelete		 should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef INCLUDE_vTaskSuspend	
	#error Missing definition:  INCLUDE_vTaskSuspend	 should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef INCLUDE_vTaskDelayUntil
	#error Missing definition:  INCLUDE_vTaskDelayUntil should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef INCLUDE_vTaskDelay
	#error Missing definition:  INCLUDE_vTaskDelay should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef configUSE_16_BIT_TICKS
	#error Missing definition:  configUSE_16_BIT_TICKS should be defined in FreeRTOSConfig.h as either 1 or 0.  See the Configuration section of the FreeRTOS API documentation for details.
#endif

#ifndef INCLUDE_xTaskGetIdleTaskHandle
	#define INCLUDE_xTaskGetIdleTaskHandle 1
#endif

#ifndef INCLUDE_xTimerGetTimerDaemonTaskHandle
	#define INCLUDE_xTimerGetTimerDaemonTaskHandle 0
#endif

#ifndef INCLUDE_pcTaskGetTaskName
	#define INCLUDE_pcTaskGetTaskName 0
#endif

#ifndef configUSE_APPLICATION_TASK_TAG
	#define configUSE_APPLICATION_TASK_TAG 0
#endif

#ifndef INCLUDE_uxTaskGetStackHighWaterMark
	#define INCLUDE_uxTaskGetStackHighWaterMark 1
#endif

#ifndef configUSE_RECURSIVE_MUTEXES
	#define configUSE_RECURSIVE_MUTEXES 0
#endif

#ifndef configUSE_MUTEXES
	#define configUSE_MUTEXES 0
#endif

#ifndef configUSE_TIMERS
	#define configUSE_TIMERS 1
#endif

#ifndef configUSE_COUNTING_SEMAPHORES
	#define configUSE_COUNTING_SEMAPHORES 1
#endif

#ifndef configUSE_MAILBOX
	#define configUSE_MAILBOX 1
#endif

#ifndef configUSE_ALTERNATIVE_API
	#define configUSE_ALTERNATIVE_API 0
#endif

#ifndef portCRITICAL_NESTING_IN_TCB
	#define portCRITICAL_NESTING_IN_TCB 0
#endif

#ifndef configMAX_TASK_NAME_LEN
	#define configMAX_TASK_NAME_LEN 16
#endif

#ifndef configIDLE_SHOULD_YIELD
	#define configIDLE_SHOULD_YIELD		1
#endif

#if configMAX_TASK_NAME_LEN < 1
	#error configMAX_TASK_NAME_LEN must be set to a minimum of 1 in FreeRTOSConfig.h
#endif

#ifndef INCLUDE_xTaskResumeFromISR
	#define INCLUDE_xTaskResumeFromISR 1
#endif

#ifndef configASSERT
	#define configASSERT( x )
#endif

/* The timers module relies on xTaskGetSchedulerState(). */
#if configUSE_TIMERS == 1

	#ifndef configTIMER_TASK_PRIORITY
		#define configTIMER_TASK_PRIORITY	1
	//	#error If configUSE_TIMERS is set to 1 then configTIMER_TASK_PRIORITY must also be defined.		
	#endif /* configTIMER_TASK_PRIORITY */

	#ifndef configTIMER_QUEUE_LENGTH
		//#error If configUSE_TIMERS is set to 1 then configTIMER_QUEUE_LENGTH must also be defined.
		#define configTIMER_QUEUE_LENGTH	128
	#endif /* configTIMER_QUEUE_LENGTH */

	#ifndef configTIMER_TASK_STACK_DEPTH
		#define configTIMER_TASK_STACK_DEPTH 200
		//#error If configUSE_TIMERS is set to 1 then configTIMER_TASK_STACK_DEPTH must also be defined.
	#endif /* configTIMER_TASK_STACK_DEPTH */

#endif /* configUSE_TIMERS */

#ifndef INCLUDE_xTaskGetSchedulerState
	#define INCLUDE_xTaskGetSchedulerState 0
#endif

#ifndef INCLUDE_xTaskGetCurrentTaskHandle
	#define INCLUDE_xTaskGetCurrentTaskHandle 0
#endif


#ifndef portSET_INTERRUPT_MASK_FROM_ISR
	#define portSET_INTERRUPT_MASK_FROM_ISR() ulSetInterruptMaskFromISR()
#endif

#ifndef portCLEAR_INTERRUPT_MASK_FROM_ISR
	#define portCLEAR_INTERRUPT_MASK_FROM_ISR( uxSavedStatusValue ) vClearInterruptMaskFromISR( uxSavedStatusValue )
#endif


#ifndef configQUEUE_REGISTRY_SIZE
	#define configQUEUE_REGISTRY_SIZE 0U
#endif

#if ( configQUEUE_REGISTRY_SIZE < 1 )
	#define vQueueAddToRegistry( xQueue, pcName )
	#define vQueueUnregisterQueue( xQueue )
#endif

#ifndef portPOINTER_SIZE_TYPE
	#define portPOINTER_SIZE_TYPE unsigned long
#endif

/* Remove any unused trace macros. */
#ifndef traceSTART
	/* Used to perform any necessary initialisation - for example, open a file
	into which trace is to be written. */
	#define traceSTART()
#endif

#ifndef traceEND
	/* Use to close a trace, for example close a file into which trace has been
	written. */
	#define traceEND()
#endif

#ifndef traceTASK_SWITCHED_IN
	/* Called after a task has been selected to run.  pxCurrentTCB holds a pointer
	to the task control block of the selected task. */
	#define traceTASK_SWITCHED_IN()
#endif

#ifndef traceTASK_SWITCHED_OUT
	/* Called before a task has been selected to run.  pxCurrentTCB holds a pointer
	to the task control block of the task being switched out. */
	#define traceTASK_SWITCHED_OUT()
#endif

#ifndef traceBLOCKING_ON_QUEUE_RECEIVE
	/* Task is about to block because it cannot read from a
	queue/mutex/semaphore.  pxQueue is a pointer to the queue/mutex/semaphore
	upon which the read was attempted.  pxCurrentTCB points to the TCB of the
	task that attempted the read. */
	#define traceBLOCKING_ON_QUEUE_RECEIVE( pxQueue )
#endif

#ifndef traceBLOCKING_ON_QUEUE_SEND
	/* Task is about to block because it cannot write to a
	queue/mutex/semaphore.  pxQueue is a pointer to the queue/mutex/semaphore
	upon which the write was attempted.  pxCurrentTCB points to the TCB of the
	task that attempted the write. */
	#define traceBLOCKING_ON_QUEUE_SEND( pxQueue )
#endif

#ifndef configCHECK_FOR_STACK_OVERFLOW
	#define configCHECK_FOR_STACK_OVERFLOW 2
#endif

/* The following event macros are embedded in the kernel API calls. */

#ifndef traceQUEUE_CREATE	
	#define traceQUEUE_CREATE( pxNewQueue )
#endif

#ifndef traceQUEUE_CREATE_FAILED
	#define traceQUEUE_CREATE_FAILED()
#endif

#ifndef traceCREATE_MUTEX
	#define traceCREATE_MUTEX( pxNewQueue )
#endif

#ifndef traceCREATE_MUTEX_FAILED
	#define traceCREATE_MUTEX_FAILED()
#endif

#ifndef traceGIVE_MUTEX_RECURSIVE
	#define traceGIVE_MUTEX_RECURSIVE( pxMutex )
#endif

#ifndef traceGIVE_MUTEX_RECURSIVE_FAILED
	#define traceGIVE_MUTEX_RECURSIVE_FAILED( pxMutex )
#endif

#ifndef traceTAKE_MUTEX_RECURSIVE
	#define traceTAKE_MUTEX_RECURSIVE( pxMutex )
#endif

#ifndef traceTAKE_MUTEX_RECURSIVE_FAILED
	#define traceTAKE_MUTEX_RECURSIVE_FAILED( pxMutex )
#endif

#ifndef traceCREATE_COUNTING_SEMAPHORE
	#define traceCREATE_COUNTING_SEMAPHORE()
#endif

#ifndef traceCREATE_COUNTING_SEMAPHORE_FAILED
	#define traceCREATE_COUNTING_SEMAPHORE_FAILED()
#endif

#ifndef traceQUEUE_SEND
	#define traceQUEUE_SEND( pxQueue )
#endif

#ifndef traceQUEUE_SEND_FAILED
	#define traceQUEUE_SEND_FAILED( pxQueue )
#endif

#ifndef traceQUEUE_RECEIVE
	#define traceQUEUE_RECEIVE( pxQueue )
#endif

#ifndef traceQUEUE_PEEK
	#define traceQUEUE_PEEK( pxQueue )
#endif

#ifndef traceQUEUE_RECEIVE_FAILED
	#define traceQUEUE_RECEIVE_FAILED( pxQueue )
#endif

#ifndef traceQUEUE_SEND_FROM_ISR
	#define traceQUEUE_SEND_FROM_ISR( pxQueue )
#endif

#ifndef traceQUEUE_SEND_FROM_ISR_FAILED
	#define traceQUEUE_SEND_FROM_ISR_FAILED( pxQueue )
#endif

#ifndef traceQUEUE_RECEIVE_FROM_ISR
	#define traceQUEUE_RECEIVE_FROM_ISR( pxQueue )
#endif

#ifndef traceQUEUE_RECEIVE_FROM_ISR_FAILED
	#define traceQUEUE_RECEIVE_FROM_ISR_FAILED( pxQueue )
#endif

#ifndef traceQUEUE_DELETE
	#define traceQUEUE_DELETE( pxQueue )
#endif

#ifndef traceTASK_CREATE
	#define traceTASK_CREATE( pxNewTCB )
#endif

#ifndef traceTASK_CREATE_FAILED
	#define traceTASK_CREATE_FAILED()
#endif

#ifndef traceTASK_DELETE
	#define traceTASK_DELETE( pxTaskToDelete )
#endif

#ifndef traceTASK_DELAY_UNTIL
	#define traceTASK_DELAY_UNTIL()
#endif

#ifndef traceTASK_DELAY
	#define traceTASK_DELAY()
#endif

#ifndef traceTASK_PRIORITY_SET
	#define traceTASK_PRIORITY_SET( pxTask, uxNewPriority )
#endif

#ifndef traceTASK_SUSPEND
	#define traceTASK_SUSPEND( pxTaskToSuspend )
#endif

#ifndef traceTASK_RESUME
	#define traceTASK_RESUME( pxTaskToResume )
#endif

#ifndef traceTASK_RESUME_FROM_ISR
	#define traceTASK_RESUME_FROM_ISR( pxTaskToResume )
#endif

#ifndef traceTASK_INCREMENT_TICK
	#define traceTASK_INCREMENT_TICK( xTickCount )
#endif

#ifndef traceTIMER_CREATE
	#define traceTIMER_CREATE( pxNewTimer )
#endif

#ifndef traceTIMER_CREATE_FAILED
	#define traceTIMER_CREATE_FAILED()
#endif

#ifndef traceTIMER_COMMAND_SEND
	#define traceTIMER_COMMAND_SEND( xTimer, xMessageID, xMessageValueValue, xReturn )
#endif

#ifndef traceTIMER_EXPIRED
	#define traceTIMER_EXPIRED( pxTimer )
#endif

#ifndef traceTIMER_COMMAND_RECEIVED
	#define traceTIMER_COMMAND_RECEIVED( pxTimer, xMessageID, xMessageValue )
#endif

#ifndef configGENERATE_RUN_TIME_STATS
	#define configGENERATE_RUN_TIME_STATS 0
#endif

#if ( configGENERATE_RUN_TIME_STATS == 1 )

	#ifndef portCONFIGURE_TIMER_FOR_RUN_TIME_STATS
		#error If configGENERATE_RUN_TIME_STATS is defined then portCONFIGURE_TIMER_FOR_RUN_TIME_STATS must also be defined.  portCONFIGURE_TIMER_FOR_RUN_TIME_STATS should call a port layer function to setup a peripheral timer/counter that can then be used as the run time counter time base.
	#endif /* portCONFIGURE_TIMER_FOR_RUN_TIME_STATS */

	#ifndef portGET_RUN_TIME_COUNTER_VALUE
		#ifndef portALT_GET_RUN_TIME_COUNTER_VALUE
			#error If configGENERATE_RUN_TIME_STATS is defined then either portGET_RUN_TIME_COUNTER_VALUE or portALT_GET_RUN_TIME_COUNTER_VALUE must also be defined.  See the examples provided and the FreeRTOS web site for more information.
		#endif /* portALT_GET_RUN_TIME_COUNTER_VALUE */
	#endif /* portGET_RUN_TIME_COUNTER_VALUE */

#endif /* configGENERATE_RUN_TIME_STATS */

#ifndef portCONFIGURE_TIMER_FOR_RUN_TIME_STATS
	#define portCONFIGURE_TIMER_FOR_RUN_TIME_STATS()
#endif

#ifndef configUSE_MALLOC_FAILED_HOOK
	#define configUSE_MALLOC_FAILED_HOOK 0
#endif

#ifndef portPRIVILEGE_BIT
	#define portPRIVILEGE_BIT ( ( unsigned portBASE_TYPE ) 0x00 )
#endif

#ifndef portYIELD_WITHIN_API
	#define portYIELD_WITHIN_API portYIELD
#endif

#ifndef pvPortMallocAligned
	#define pvPortMallocAligned( x, puxStackBuffer ) ( ( ( puxStackBuffer ) == NULL ) ? ( pvPortMalloc( ( x ) ) ) : ( puxStackBuffer ) )
#endif

#ifndef vPortFreeAligned
	#define vPortFreeAligned( pvBlockToFree ) if (xPortMemIsKernel(pvBlockToFree)) vPortFree( pvBlockToFree )
#endif

#endif /* INC_FREERTOS_H */

