(module PinHeader_1x05_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 5E31BC37)
  (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
  (tags "Through hole angled pin header THT 1x05 2.54mm single row")
  (fp_text reference REF** (at 4.385 -2.27) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PinHeader_1x05_P2.54mm_Horizontal_SMD (at 4.385 12.43) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 2.77 5.08 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 10.55 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.55 11.95) (end 10.55 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 11.95) (end 10.55 11.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 -1.8) (end -1.8 11.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 0) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.042929 10.54) (end 1.44 10.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.042929 9.78) (end 1.44 9.78) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 10.54) (end 4.1 10.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 9.78) (end 10.1 10.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 9.78) (end 10.1 9.78) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.44 8.89) (end 4.1 8.89) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.042929 8) (end 1.44 8) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.042929 7.24) (end 1.44 7.24) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 8) (end 4.1 8) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 7.24) (end 10.1 8) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 7.24) (end 10.1 7.24) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.44 6.35) (end 4.1 6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.042929 5.46) (end 1.44 5.46) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.042929 4.7) (end 1.44 4.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 5.46) (end 4.1 5.46) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 4.7) (end 10.1 5.46) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 4.7) (end 10.1 4.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.44 3.81) (end 4.1 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.042929 2.92) (end 1.44 2.92) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.042929 2.16) (end 1.44 2.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 2.92) (end 4.1 2.92) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 2.16) (end 10.1 2.92) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 2.16) (end 10.1 2.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.44 1.27) (end 4.1 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 0.28) (end 10.1 0.28) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 0.16) (end 10.1 0.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 0.04) (end 10.1 0.04) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 -0.08) (end 10.1 -0.08) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 -0.2) (end 10.1 -0.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 -0.32) (end 10.1 -0.32) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 0.38) (end 4.1 0.38) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.1 -0.38) (end 10.1 0.38) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 -0.38) (end 10.1 -0.38) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 -1.33) (end 1.44 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.1 11.49) (end 4.1 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.44 11.49) (end 4.1 11.49) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.44 -1.33) (end 1.44 11.49) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.04 10.48) (end 10.04 10.48) (layer F.Fab) (width 0.1))
  (fp_line (start 10.04 9.84) (end 10.04 10.48) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 9.84) (end 10.04 9.84) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 10.48) (end 1.5 10.48) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 9.84) (end -0.32 10.48) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 9.84) (end 1.5 9.84) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 7.94) (end 10.04 7.94) (layer F.Fab) (width 0.1))
  (fp_line (start 10.04 7.3) (end 10.04 7.94) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 7.3) (end 10.04 7.3) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 7.94) (end 1.5 7.94) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 7.3) (end 1.5 7.3) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 5.4) (end 10.04 5.4) (layer F.Fab) (width 0.1))
  (fp_line (start 10.04 4.76) (end 10.04 5.4) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 4.76) (end 10.04 4.76) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 5.4) (end 1.5 5.4) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 4.76) (end 1.5 4.76) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 2.86) (end 10.04 2.86) (layer F.Fab) (width 0.1))
  (fp_line (start 10.04 2.22) (end 10.04 2.86) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 2.22) (end 10.04 2.22) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 2.86) (end 1.5 2.86) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 2.22) (end 1.5 2.22) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
  (fp_line (start 10.04 -0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
  (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -0.635) (end 2.135 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 11.43) (end 1.5 -0.635) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 11.43) (end 1.5 11.43) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 -1.27) (end 4.04 11.43) (layer F.Fab) (width 0.1))
  (fp_line (start 2.135 -1.27) (end 4.04 -1.27) (layer F.Fab) (width 0.1))
  (pad 5 smd rect (at 0 10.16) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0 7.62) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 5.08) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 2.54) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0 0) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
